

Latency: 8 clock cycles

Throughput = 1/8

Registers: 3

Output: 1

Input: 4

Adders: 3

Maxers: 1

Multipliers: 1

Subtractors: 1

Clock period = flop + maxer + maximum\_of(3\*adder, multiplier)